; Copyright (c) 1999-2001 SigmaTel Inc.

[Version]
Signature="$CHICAGO$"
Class=MEDIA
ClassGUID={4d36e96c-e325-11ce-bfc1-08002be10318}
provider=%SGTML%
DriverVer=08/11/2002, 5.10.00.3686
CatalogFile=stac97.cat

[SourceDisksNames]
222="AC97 WDM SigmaTel Driver Disk",,,

[SourceDisksFiles]
stac97.sys=222
stac97.cpl=222

[Manufacturer]
%SgtmlMfg%=SigmaTel

[SigmaTel]
;SigmaTel Default Settings
%STAC97.DeviceDescSis961%=STAC97, PCI\VEN_1039&DEV_7012&subsys_20071631
%STAC97.DeviceDescSis961%=STAC97, PCI\VEN_1039&DEV_7012&subsys_001317C0

;Customer Specific Settings
%STAC97.DeviceDescSis961%=STAC97_11C910CF, PCI\VEN_1039&DEV_7012&subsys_11C910CF
%STAC97.DeviceDescSis961%=STAC97_70121054, PCI\VEN_1039&DEV_7012&subsys_70121054
%STAC97.DeviceDescSis961%=STAC97_001814C0, PCI\VEN_1039&DEV_7012&subsys_001814C0
%STAC97.DeviceDescSis961%=STAC97_001814C0, PCI\VEN_1039&DEV_7012&subsys_001514C0

%STAC97.DeviceDescSis961%=STAC97_10101734, PCI\VEN_1039&DEV_7012&SUBSYS_10101734

;SigmaTel ID's
;SiS961
%STAC97.DeviceDescSis961%=STAC97, PCI\VEN_1039&DEV_7012&subsys_76008384 ;9700
%STAC97.DeviceDescSis961%=STAC97, PCI\VEN_1039&DEV_7012&subsys_76088384 ;9708
%STAC97.DeviceDescSis961%=STAC97, PCI\VEN_1039&DEV_7012&subsys_76098384 ;9721
%STAC97.DeviceDescSis961%=STAC97, PCI\VEN_1039&DEV_7012&subsys_76448384 ;9744
%STAC97.DeviceDescSis961%=STAC97, PCI\VEN_1039&DEV_7012&subsys_76568384 ;9756
%STAC97.DeviceDescSis961%=STAC97, PCI\VEN_1039&DEV_7012&subsys_76508384 ;9750
%STAC97.DeviceDescSis961%=STAC97, PCI\VEN_1039&DEV_7012&subsys_76528384 ;9752
%STAC97.DeviceDescSis961%=STAC97, PCI\VEN_1039&DEV_7012&subsys_76668384 ;9766

[DestinationDirs]
STAC97.CopyList=10,system32\drivers
STAC97.CopyList1=11

;*********************** SigmaTel Specific Settings ******************************
;Affects only Generic Drivers
;
[STAC97]
AlsoInstall=ks.registration(ks.inf),wdmaudio.registration(wdmaudio.inf)
CopyFiles=STAC97.CopyList
AddReg=STAC97.AddReg, STAC97Names.AddReg, STAC97_MC.AddReg, STAC97_MD.AddReg
DelReg=STAC97.DelReg
DriverVer=08/11/2002, 5.10.00.3686

[STAC97.nt]
Include=LayoutFile=layout.inf,ks.inf,wdmaudio.inf
Needs=KS.Registration,WDMAUDIO.Registration
CopyFiles=STAC97.CopyList
AddReg=STAC97.AddReg, STAC97Names.AddReg, STAC97_MC.AddReg, STAC97_MD.AddReg
DelReg=STAC97.DelReg
DriverVer=08/11/2002, 5.10.00.3686

[STAC97.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AlternateWave%,STAC97.Interface.AlternateWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AlternateWave%,STAC97.Interface.AlternateWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%,STAC97.Interface.Topology
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_UART%,STAC97.Interface.UART
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_UART%,STAC97.Interface.UART
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_UART%,STAC97.Interface.UART

[STAC97.nt.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AlternateWave%,STAC97.Interface.AlternateWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AlternateWave%,STAC97.Interface.AlternateWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%,STAC97.Interface.Topology
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_UART%,STAC97.Interface.UART
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_UART%,STAC97.Interface.UART
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_UART%,STAC97.Interface.UART

[STAC97.Services]
AddService = STAC97, 0x00000002, STAC97_Service_Inst

[STAC97.nt.Services]
AddService = STAC97, 0x00000002, STAC97_Service_Inst

[STAC97_MD.AddReg]
;This section is for resolving conflicts with registry settings

;*********************** END SigmaTel Specific Settings ************************

;***********************Vendor 10101734 Specific Settings***********************
;Affects only Vendor 10101734
;
[STAC97_10101734]
AlsoInstall=ks.registration(ks.inf),wdmaudio.registration(wdmaudio.inf)
CopyFiles=STAC97.CopyList
AddReg=STAC97.AddReg, STAC97Names.AddReg, STAC97_MC.AddReg, STAC97_10101734.AddReg
DelReg=STAC97.DelReg
DriverVer=08/11/2002, 5.10.00.3686

[STAC97_10101734.nt]
Include=LayoutFile=layout.inf,ks.inf,wdmaudio.inf
Needs=KS.Registration,WDMAUDIO.Registration
CopyFiles=STAC97.CopyList
AddReg=STAC97.AddReg, STAC97Names.AddReg, STAC97_MC.AddReg, STAC97_10101734.AddReg
DelReg=STAC97.DelReg
DriverVer=08/11/2002, 5.10.00.3686

[STAC97_10101734.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AlternateWave%,STAC97.Interface.AlternateWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AlternateWave%,STAC97.Interface.AlternateWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%,STAC97.Interface.Topology
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_UART%,STAC97.Interface.UART
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_UART%,STAC97.Interface.UART
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_UART%,STAC97.Interface.UART

[STAC97_10101734.nt.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AlternateWave%,STAC97.Interface.AlternateWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AlternateWave%,STAC97.Interface.AlternateWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%,STAC97.Interface.Topology
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_UART%,STAC97.Interface.UART
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_UART%,STAC97.Interface.UART
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_UART%,STAC97.Interface.UART

[STAC97_10101734.Services]
AddService = STAC97, 0x00000002, STAC97_Service_Inst

[STAC97_10101734.nt.Services]
AddService = STAC97, 0x00000002, STAC97_Service_Inst

[STAC97_10101734.AddReg]

HKR,%MixerDefaultsSubKeyName%,DisableWaveIn2,                      1, 1
HKR,%MixerDefaultsSubKeyName%,MasterMute,                          1, 0                    ; 0, unmuted, 1 muted
HKR,%ConfigurationsSubKeyName%,FadeAudio,                        1, 0
HKR,%ConfigurationsSubKeyName%,ActiveMuteDelayEnabled,           1, 0     ; If FadeAudio, zipper noise mute of PCM is deferred until signal fade has completed.
HKR,%ConfigurationsSubKeyName%,EnableExtAmpControl,                1, 1
HKR,%ConfigurationsSubKeyName%,ExtAmpPops,                         1,1
HKR,%ConfigurationsSubKeyName%,ExtAmpPowerUpOnSystemSuspend,       1,1
HKR,%ConfigurationsSubKeyName%,ExtAmpPowerDownTimeInMCS,           0x00010001, 5000 
HKR,%ConfigurationsSubKeyName%,ExtAmpPowerUpTimeInMCS,             0x00010001, 5000
HKR,%ConfigurationsSubKeyName%,CodecPowerUpDelayInMCS,             0x00010001, 1000

HKR,%MixerDefaultsSubKeyName%,MasterVolume,                      1, 00, 00, f9, ff ; 0404 r02
HKR,%MixerDefaultsSubKeyName%,HeadphoneVolume,                   1, 00, 00, f9, ff ; 0404 r04
HKR,%MixerDefaultsSubKeyName%,LnlvlVolume,                       1, 00, 00, f9, ff ; 0404 r04
HKR,%MixerDefaultsSubKeyName%,MonoMixerAtMonoOutVolume,          1, 00, 00, f9, ff ; 0004 r06
HKR,%MixerDefaultsSubKeyName%,PCBeepVolume,                      1, 00, 00, 00, 00 ; 0000
HKR,%ConfigurationsSubKeyName%,PCMVolumeFixedLevel,              1, 07, 07
HKR,%MixerDefaultsSubKeyName%,VideoVolume,                       1, 00, 01, 0c, 00 ; 0000 +12dB
HKR,%MixerDefaultsSubKeyName%,LineInMute,                        1, 0

HKR,%MixerDefaultsSubKeyName%,PhoneMute,                         1, 1
HKR,%MixerDefaultsSubKeyName%,AuxMute,                           1, 1
HKR,%MixerDefaultsSubKeyName%,VideoMute,                         1, 1

HKR,%MixerDefaultsSubKeyName%,WaveInMux,                         1, 00, 00, 00, 00       ; WaveInMux selection values: (0: MIC), (1: CD), (2: Video), (3: Aux), (4: LineIn), (5: StereoMix), (6: MonoMix), (7: Phone).
HKR,%MixerDefaultsSubKeyName%,PhoneAtRecMuxVolume,               1, 00, 81, 04, 00       ; 0303
HKR,%MixerDefaultsSubKeyName%,MICAtRecMuxVolume,                 1, 00, 81, 04, 00       ; 0303
HKR,%MixerDefaultsSubKeyName%,CDAtRecMuxVolume,                  1, 00, 81, 04, 00       ; 0303
HKR,%MixerDefaultsSubKeyName%,VideoAtRecMuxVolume,               1, 00, 81, 04, 00       ; 0303
HKR,%MixerDefaultsSubKeyName%,AuxAtRecMuxVolume,                 1, 00, 81, 04, 00       ; 0303
HKR,%MixerDefaultsSubKeyName%,LineInAtRecMuxVolume,              1, 00, 81, 04, 00       ; 0303
HKR,%MixerDefaultsSubKeyName%,StereoMixAtRecMuxVolume,           1, 00, 81, 04, 00       ; 0303
HKR,%MixerDefaultsSubKeyName%,MonoMixAtRecMuxVolume,             1, 00, 81, 04, 00       ; 0303

HKR,%MixerDefaultsSubKeyName%,MonoOutMux,                        1, 00, 00, 00, 00       ; MonoOutMux selection values: (0: MIC), (1: MonoMix).
HKR,%MixerDefaultsSubKeyName%,DisableMonoOut,                    1, 01

HKR,%ConfigurationsSubKeyName%,OverridePowerSupplyVoltageAutoDetect, 1, 1
HKR,%ConfigurationsSubKeyName%,PowerSupplyVoltageIs5V, 1, 1 ; 5V
HKR,%ConfigurationsSubKeyName%,EnableVRA, 1, 1
HKR,%ConfigurationsSubKeyName%,ADCVRADisables, 0x00010001, 254 ; 48
HKR,%ConfigurationsSubKeyName%,DACVRADisables, 0x00010001, 248 ; 48, 44.1, 32

HKR,%MixerDefaultsSubKeyName%,CPL_SpdifTransmitterEnabledByUser, 1, 1
HKR,%ConfigurationsSubKeyName%,DisableSPDIFControl,1,0

HKR,%MixerDefaultsSubKeyName%,DisablePCBeep,                     1, 1
; HKR,%MixerDefaultsSubKeyName%,DisablePhone,                      1, 1
; HKR,%MixerDefaultsSubKeyName%,DisableMIC,                        1, 1
; HKR,%MixerDefaultsSubKeyName%,DisableLineIn,                     1, 1
; HKR,%MixerDefaultsSubKeyName%,DisableCDIn,                       1, 1
; HKR,%MixerDefaultsSubKeyName%,DisableVideo,                      1, 1
; HKR,%MixerDefaultsSubKeyName%,DisableAux,                        1, 1
HKR,%MixerDefaultsSubKeyName%,DisableSurround,                   1, 1
HKR,%MixerDefaultsSubKeyName%,DisableCenter,                     1, 1
HKR,%MixerDefaultsSubKeyName%,DisableLFE,                        1, 1
HKR,%MixerDefaultsSubKeyName%,DisableStereo2Virtual,             1, 1
HKR,%MixerDefaultsSubKeyName%,DisableMono2Virtual,               1, 1
HKR,%MixerDefaultsSubKeyName%,DisableWaveIn2,                    1, 1
HKR,%MixerDefaultsSubKeyName%,MICBoost,                            1, 1
HKR,%ConfigurationsSubKeyName%,EnableNonPCMOnWin2K,                1, 1
HKR,%ConfigurationsSubKeyName%,MasterControlsAux,                1, 1
HKR,%ConfigurationsSubKeyName%,MasterControlsMono,               1, 1

; HKR,%ConfigurationsSubKeyName%,UseAltNameForPcBeep, 1, 1

;*********************** END Vendor 10101734 Specific Settings******************


;***********************Vendor 11C910CF Specific Settings***********************
;Affects only Vendor 11C910CF
;
[STAC97_11C910CF]
AlsoInstall=ks.registration(ks.inf),wdmaudio.registration(wdmaudio.inf)
CopyFiles=STAC97.CopyList,STAC97.CopyList1
AddReg=STAC97.AddReg, STAC97Names.AddReg, STAC97_MC.AddReg, STAC97_11C910CF.AddReg
DelReg=STAC97.DelReg
DriverVer=08/11/2002, 5.10.00.3686

[STAC97_11C910CF.nt]
Include=LayoutFile=layout.inf,ks.inf,wdmaudio.inf
Needs=KS.Registration,WDMAUDIO.Registration
CopyFiles=STAC97.CopyList,STAC97.CopyList1
AddReg=STAC97.AddReg, STAC97Names.AddReg, STAC97_MC.AddReg, STAC97_11C910CF.AddReg
DelReg=STAC97.DelReg
DriverVer=08/11/2002, 5.10.00.3686

[STAC97_11C910CF.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AlternateWave%,STAC97.Interface.AlternateWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AlternateWave%,STAC97.Interface.AlternateWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%,STAC97.Interface.Topology
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_UART%,STAC97.Interface.UART
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_UART%,STAC97.Interface.UART
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_UART%,STAC97.Interface.UART

[STAC97_11C910CF.nt.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AlternateWave%,STAC97.Interface.AlternateWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AlternateWave%,STAC97.Interface.AlternateWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%,STAC97.Interface.Topology
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_UART%,STAC97.Interface.UART
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_UART%,STAC97.Interface.UART
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_UART%,STAC97.Interface.UART

[STAC97_11C910CF.Services]
AddService = STAC97, 0x00000002, STAC97_Service_Inst

[STAC97_11C910CF.nt.Services]
AddService = STAC97, 0x00000002, STAC97_Service_Inst

[STAC97_11C910CF.AddReg]

HKR,%MixerDefaultsSubKeyName%,DisableWaveIn2,                      1, 1
HKR,%MixerDefaultsSubKeyName%,MasterMute,                          1, 0                    ; 0, unmuted, 1 muted
HKR,%ConfigurationsSubKeyName%,FadeAudio,                        1, 0
HKR,%ConfigurationsSubKeyName%,ActiveMuteDelayEnabled,           1, 0     ; If FadeAudio, zipper noise mute of PCM is deferred until signal fade has completed.
HKR,%ConfigurationsSubKeyName%,EnableExtAmpControl,                1, 1
HKR,%ConfigurationsSubKeyName%,ExtAmpPops,                         1,1
HKR,%ConfigurationsSubKeyName%,ExtAmpPowerUpOnSystemSuspend,       1,1
HKR,%ConfigurationsSubKeyName%,ExtAmpPowerDownTimeInMCS,           0x00010001, 5000 
HKR,%ConfigurationsSubKeyName%,ExtAmpPowerUpTimeInMCS,             0x00010001, 5000
HKR,%ConfigurationsSubKeyName%,CodecPowerUpDelayInMCS,             0x00010001, 1000

HKR,%MixerDefaultsSubKeyName%,MasterVolume,                      1, 00, 00, f9, ff ; 0404 r02
HKR,%MixerDefaultsSubKeyName%,HeadphoneVolume,                   1, 00, 00, f9, ff ; 0404 r04
HKR,%MixerDefaultsSubKeyName%,LnlvlVolume,                       1, 00, 00, f9, ff ; 0404 r04
HKR,%MixerDefaultsSubKeyName%,MonoMixerAtMonoOutVolume,          1, 00, 00, f9, ff ; 0004 r06
HKR,%MixerDefaultsSubKeyName%,PCBeepVolume,                      1, 00, 00, 00, 00 ; 0000
HKR,%ConfigurationsSubKeyName%,PCMVolumeFixedLevel,              1, 07, 07
HKR,%MixerDefaultsSubKeyName%,VideoVolume,                       1, 00, 01, 0c, 00 ; 0000 +12dB
HKR,%MixerDefaultsSubKeyName%,LineInMute,                        1, 0
HKR,%MixerDefaultsSubKeyName%,PhoneMute,                         1, 0

HKR,%MixerDefaultsSubKeyName%,WaveInMux,                         1, 00, 00, 00, 00       ; WaveInMux selection values: (0: MIC), (1: CD), (2: Video), (3: Aux), (4: LineIn), (5: StereoMix), (6: MonoMix), (7: Phone).
HKR,%MixerDefaultsSubKeyName%,PhoneAtRecMuxVolume,               1, 00, 81, 04, 00       ; 0303
HKR,%MixerDefaultsSubKeyName%,MICAtRecMuxVolume,                 1, 00, 81, 04, 00       ; 0303
HKR,%MixerDefaultsSubKeyName%,CDAtRecMuxVolume,                  1, 00, 81, 04, 00       ; 0303
HKR,%MixerDefaultsSubKeyName%,VideoAtRecMuxVolume,               1, 00, 81, 04, 00       ; 0303
HKR,%MixerDefaultsSubKeyName%,AuxAtRecMuxVolume,                 1, 00, 81, 04, 00       ; 0303
HKR,%MixerDefaultsSubKeyName%,LineInAtRecMuxVolume,              1, 00, 81, 04, 00       ; 0303
HKR,%MixerDefaultsSubKeyName%,StereoMixAtRecMuxVolume,           1, 00, 81, 04, 00       ; 0303
HKR,%MixerDefaultsSubKeyName%,MonoMixAtRecMuxVolume,             1, 00, 81, 04, 00       ; 0303

HKR,%MixerDefaultsSubKeyName%,MonoOutMux,                        1, 00, 00, 00, 00       ; MonoOutMux selection values: (0: MIC), (1: MonoMix).

HKR,%ConfigurationsSubKeyName%,OverridePowerSupplyVoltageAutoDetect, 1, 1
HKR,%ConfigurationsSubKeyName%,PowerSupplyVoltageIs5V, 1, 1 ; 5V
HKR,%ConfigurationsSubKeyName%,EnableVRA, 1, 1
HKR,%ConfigurationsSubKeyName%,ADCVRADisables, 0x00010001, 254 ; 48
HKR,%ConfigurationsSubKeyName%,DACVRADisables, 0x00010001, 248 ; 48, 44.1, 32

HKR,%ConfigurationsSubKeyName%,CPL_SaveExtraPower,1,0
HKR,%ConfigurationsSubKeyName%,CPL_SecondsAfter,0x00010001,30
HKR,%ConfigurationsSubKeyName%,CPL_MaySwitchExtAmpPowerState,1,0
HKR,%ConfigurationsSubKeyName%,CPL_UserControlsMaySwitchExtAmpPowerState,1,1
HKR,%ConfigurationsSubKeyName%,CPL_UserControlsPowerManagementSettings,1,0
HKR,%ConfigurationsSubKeyName%,CPL_FixedDigitalOutRate,0x00010001,0 ; "dynamic"
HKR,%ConfigurationsSubKeyName%,CPL_UserControlsFixedDigitalOutRate, 1, 1
HKR,%MixerDefaultsSubKeyName%,CPL_SpdifTransmitterEnabledByUser, 1, 1
HKR,%ConfigurationsSubKeyName%,DisableSPDIFControl,1,1
HKR,%ConfigurationsSubKeyName%,EnableNonPCMOnWin2K,                1, 1

; HKR,%MixerDefaultsSubKeyName%,DisablePCBeep,                     1, 1
; HKR,%MixerDefaultsSubKeyName%,DisablePhone,                      1, 1
; HKR,%MixerDefaultsSubKeyName%,DisableMIC,                        1, 1
; HKR,%MixerDefaultsSubKeyName%,DisableLineIn,                     1, 1
; HKR,%MixerDefaultsSubKeyName%,DisableCDIn,                       1, 1
; HKR,%MixerDefaultsSubKeyName%,DisableVideo,                      1, 1
HKR,%MixerDefaultsSubKeyName%,DisableAux,                        1, 1
HKR,%MixerDefaultsSubKeyName%,DisableSurround,                   1, 1
HKR,%MixerDefaultsSubKeyName%,DisableCenter,                     1, 1
HKR,%MixerDefaultsSubKeyName%,DisableLFE,                        1, 1
HKR,%MixerDefaultsSubKeyName%,DisableStereo2Virtual,             1, 1
HKR,%MixerDefaultsSubKeyName%,DisableMono2Virtual,               1, 1
HKR,%MixerDefaultsSubKeyName%,DisableWaveIn2,                    1, 1

HKR,%ConfigurationsSubKeyName%,UseAltNameForPcBeep, 1, 1

;*********************** END Vendor 11C910CF Specific Settings******************


;***********************Vendor 70121054 Specific Settings***********************
;Affects only Vendor 70121054
;
[STAC97_70121054]
AlsoInstall=ks.registration(ks.inf),wdmaudio.registration(wdmaudio.inf)
CopyFiles=STAC97.CopyList
AddReg=STAC97.AddReg, STAC97Names.AddReg, STAC97_MC.AddReg, STAC97_70121054.AddReg
DelReg=STAC97.DelReg
DriverVer=08/11/2002, 5.10.00.3686

[STAC97_70121054.nt]
Include=LayoutFile=layout.inf,ks.inf,wdmaudio.inf
Needs=KS.Registration,WDMAUDIO.Registration
CopyFiles=STAC97.CopyList
AddReg=STAC97.AddReg, STAC97Names.AddReg, STAC97_MC.AddReg, STAC97_70121054.AddReg
DelReg=STAC97.DelReg
DriverVer=08/11/2002, 5.10.00.3686

[STAC97_70121054.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AlternateWave%,STAC97.Interface.AlternateWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AlternateWave%,STAC97.Interface.AlternateWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%,STAC97.Interface.Topology
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_UART%,STAC97.Interface.UART
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_UART%,STAC97.Interface.UART
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_UART%,STAC97.Interface.UART

[STAC97_70121054.nt.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AlternateWave%,STAC97.Interface.AlternateWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AlternateWave%,STAC97.Interface.AlternateWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%,STAC97.Interface.Topology
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_UART%,STAC97.Interface.UART
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_UART%,STAC97.Interface.UART
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_UART%,STAC97.Interface.UART

[STAC97_70121054.Services]
AddService = STAC97, 0x00000002, STAC97_Service_Inst

[STAC97_70121054.nt.Services]
AddService = STAC97, 0x00000002, STAC97_Service_Inst

[STAC97_70121054.AddReg]
HKR,%ConfigurationsSubKeyName%,DCRecordBias,                   1, 7F, 00, 00, 00

;*********************** END Vendor 70121054 Specific Settings******************

;***********************Vendor 001814C0 Specific Settings***********************
;Affects only Vendor 001814C0
;
[STAC97_001814C0]
AlsoInstall=ks.registration(ks.inf),wdmaudio.registration(wdmaudio.inf)
CopyFiles=STAC97.CopyList
AddReg=STAC97.AddReg, STAC97Names.AddReg, STAC97_MC.AddReg, STAC97_001814C0.AddReg
DriverVer=08/11/2002, 5.10.00.3686

[STAC97_001814C0.nt]
Include=LayoutFile=layout.inf,ks.inf,wdmaudio.inf
Needs=KS.Registration,WDMAUDIO.Registration
CopyFiles=STAC97.CopyList
AddReg=STAC97.AddReg, STAC97Names.AddReg, STAC97_MC.AddReg, STAC97_001814C0.AddReg
DriverVer=08/11/2002, 5.10.00.3686

[STAC97_001814C0.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AlternateWave%,STAC97.Interface.AlternateWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AlternateWave%,STAC97.Interface.AlternateWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%,STAC97.Interface.Topology
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_UART%,STAC97.Interface.UART
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_UART%,STAC97.Interface.UART
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_UART%,STAC97.Interface.UART

[STAC97_001814C0.nt.Interfaces]
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_Wave%,STAC97.Interface.Wave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_AlternateWave%,STAC97.Interface.AlternateWave
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_AlternateWave%,STAC97.Interface.AlternateWave
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_Topology%,STAC97.Interface.Topology
AddInterface=%KSCATEGORY_AUDIO%,%KSNAME_UART%,STAC97.Interface.UART
AddInterface=%KSCATEGORY_RENDER%,%KSNAME_UART%,STAC97.Interface.UART
AddInterface=%KSCATEGORY_CAPTURE%,%KSNAME_UART%,STAC97.Interface.UART

[STAC97_001814C0.Services]
AddService = STAC97, 0x00000002, STAC97_Service_Inst

[STAC97_001814C0.nt.Services]
AddService = STAC97, 0x00000002, STAC97_Service_Inst

[STAC97_001814C0.AddReg]
HKR,%MixerDefaultsSubKeyName%,WaveInMux,                         1, 00, 00, 00, 00       ; WaveInMux selection values: (0: MIC), (1: CD), (2: Video), (3: Aux), (4: LineIn), (5: StereoMix), (6: MonoMix), (7: Phone).
;*********************** END Vendor 001814C0 Specific Settings******************


;******************************** Common *****************************************
;Affects all drivers

[STAC97.CopyList]
STAC97.sys

[STAC97.CopyList1]
STAC97.cpl

[STAC97.Interface.Wave]
AddReg=STAC97.I.Wave.AddReg

[STAC97.I.Wave.AddReg]
HKR,,CLSID,,%Proxy.CLSID%
HKR,,FriendlyName,,%STAC97.Wave.szPname%

[STAC97.Interface.AlternateWave]
AddReg=STAC97.I.AlternateWave.AddReg

[STAC97.I.AlternateWave.AddReg]
HKR,,CLSID,,%Proxy.CLSID%
HKR,,FriendlyName,,%STAC97.AlternateWave.szPname%

[STAC97.Interface.Topology]
AddReg=STAC97.I.Topo.AddReg

[STAC97.I.Topo.AddReg]
HKR,,CLSID,,%Proxy.CLSID%
HKR,,FriendlyName,,%STAC97.Topology.szPname%

[STAC97.Interface.UART]
AddReg=STAC97.Interface.UART.AddReg
[STAC97.Interface.UART.AddReg]
HKR,,CLSID,,%Proxy.CLSID%
HKR,,FriendlyName,,%STAC97.UART.szPname%

[STAC97.DelReg]
HKCU,%SndVolSigKey%
HKU,%SndVolSigKey%

[STAC97.AddReg]
HKR,,AssociatedFilters,,"wdmaud,swmidi,redbook"
HKR,,Driver,,STAC97.sys
HKR,,NTMPDriver,,"STAC97.sys,sbemul.sys"

HKR,Drivers,SubClasses,,"wave,midi,mixer"

HKR,Drivers\wave\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\midi\wdmaud.drv,Driver,,wdmaud.drv
HKR,Drivers\mixer\wdmaud.drv,Driver,,wdmaud.drv

HKR,Drivers\wave\wdmaud.drv,Description,,%STAC97.DeviceDesc%
HKR,Drivers\midi\wdmaud.drv, Description,,%WDM_MIDI%
HKR,Drivers\mixer\wdmaud.drv,Description,,%STAC97.DeviceDesc%

[STAC97_Service_Inst]
DisplayName   = %STAC97.SvcDesc%
ServiceType   = 1                  ; SERVICE_KERNEL_DRIVER
StartType     = 3                  ; SERVICE_DEMAND_START
ErrorControl  = 1                  ; SERVICE_ERROR_NORMAL
ServiceBinary = %10%\system32\drivers\STAC97.sys

[STAC97Names.AddReg]
;; Nodes
HKLM,%MediaCategories%\%STAC97GUID.PhoneVolume%,Name,,%STAC97Node.PhoneVolume%
HKLM,%MediaCategories%\%STAC97GUID.PhoneVolume%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.PhoneMute%,Name,,%STAC97Node.PhoneMute%
HKLM,%MediaCategories%\%STAC97GUID.PhoneMute%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.LineInMute%,Name,,%STAC97Node.LineInMute%
HKLM,%MediaCategories%\%STAC97GUID.LineInMute%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.MainMix%,Name,,%STAC97Node.MainMix%
HKLM,%MediaCategories%\%STAC97GUID.MainMix%,Display,1,00,00,00,00
;HKLM,%MediaCategories%\%STAC97GUID.Virt3DCenter%,Name,,%STAC97Node.Virt3DCenter%
;HKLM,%MediaCategories%\%STAC97GUID.Virt3DCenter%,Display,1,00,00,00,00
;HKLM,%MediaCategories%\%STAC97GUID.Virt3DDepth%,Name,,%STAC97Node.Virt3DDepth%
;HKLM,%MediaCategories%\%STAC97GUID.Virt3DDepth%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.3DBypass%,Name,,%STAC97Node.3DBypass%
HKLM,%MediaCategories%\%STAC97GUID.3DBypass%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.3DEnable%,Name,,%STAC97Node.3DEnable%
HKLM,%MediaCategories%\%STAC97GUID.3DEnable%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.BeepMix%,Name,,%STAC97Node.BeepMix%
HKLM,%MediaCategories%\%STAC97GUID.BeepMix%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.HPVolume%,Name,,%STAC97Node.HPVolume%
HKLM,%MediaCategories%\%STAC97GUID.HPVolume%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.HPMute%,Name,,%STAC97Node.HPMute%
HKLM,%MediaCategories%\%STAC97GUID.HPMute%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.LnlvlVolume%,Name,,%STAC97Node.LnlvlVolume%
HKLM,%MediaCategories%\%STAC97GUID.LnlvlVolume%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.LnlvlMute%,Name,,%STAC97Node.LnlvlMute%
HKLM,%MediaCategories%\%STAC97GUID.LnlvlMute%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.MonoOutSelect%,Name,,%STAC97Node.MonoOutSelect%
HKLM,%MediaCategories%\%STAC97GUID.MonoOutSelect%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.WaveInSelect%,Name,,%STAC97Node.WaveInSelect%
HKLM,%MediaCategories%\%STAC97GUID.WaveInSelect%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.MasterInVolume%,Name,,%STAC97Node.MasterInVolume%
HKLM,%MediaCategories%\%STAC97GUID.MasterInVolume%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.MasterInMute%,Name,,%STAC97Node.MasterInMute%
HKLM,%MediaCategories%\%STAC97GUID.MasterInMute%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.MicInVolume%,Name,,%STAC97Node.MicInVolume%
HKLM,%MediaCategories%\%STAC97GUID.MicInVolume%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.MicInMute%,Name,,%STAC97Node.MicInMute%
HKLM,%MediaCategories%\%STAC97GUID.MicInMute%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.SurroundVolume%,Name,,%STAC97Node.SurroundVolume%
HKLM,%MediaCategories%\%STAC97GUID.SurroundVolume%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.SurroundMute%,Name,,%STAC97Node.SurroundMute%
HKLM,%MediaCategories%\%STAC97GUID.SurroundMute%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.CenterVolume%,Name,,%STAC97Node.CenterVolume%
HKLM,%MediaCategories%\%STAC97GUID.CenterVolume%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.CenterMute%,Name,,%STAC97Node.CenterMute%
HKLM,%MediaCategories%\%STAC97GUID.CenterMute%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.LFEVolume%,Name,,%STAC97Node.LFEVolume%
HKLM,%MediaCategories%\%STAC97GUID.LFEVolume%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.LFEMute%,Name,,%STAC97Node.LFEMute%
HKLM,%MediaCategories%\%STAC97GUID.LFEMute%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.DigitalEnable%,Name,,%STAC97Node.DigitalEnable%
HKLM,%MediaCategories%\%STAC97GUID.MultiChannelEnable%,Name,,%STAC97Node.MultiChannelEnable%
HKLM,%MediaCategories%\%STAC97GUID.GPIOControl%,Name,,%STAC97Node.GPIOControl%
HKLM,%MediaCategories%\%STAC97GUID.HPOutPin%,Name,,%STAC97Pin.HPOutPin%
HKLM,%MediaCategories%\%STAC97GUID.HPOutPin%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.LnlvlOutPin%,Name,,%STAC97Pin.LnlvlOutPin%
HKLM,%MediaCategories%\%STAC97GUID.LnlvlOutPin%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.Mic2Pin%,Name,,%STAC97Pin.Mic2Pin%
HKLM,%MediaCategories%\%STAC97GUID.Mic2Pin%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.LineIn2Pin%,Name,,%STAC97Pin.LineIn2Pin%
HKLM,%MediaCategories%\%STAC97GUID.LineIn2Pin%,Display,1,00,00,00,00
HKLM,%MediaCategories%\%STAC97GUID.MonoMuteInMasterAdvanced%,Name,,%STAC97Node.MonoMuteInMasterAdvanced%
HKLM,%MediaCategories%\%STAC97GUID_ALTNAME.PcSpeaker%,Name,,%STAC97Pin.PcSpeaker%
HKLM,%MediaCategories%\%STAC97GUID_ALTNAME.PcSpeaker%,Display,1,00,00,00,00

[STAC97_MC.AddReg]
;
;   Model common data.
;
;   Default register value at driver startup
;   Uncomment some one of the lines if you want to overwrite the default setting
;   The value in these outcommented lines is the driver default. You can change
;   the register values (and uncomment the line) to overwrite the driver default.
;   low byte comes first, values are hexadecimal.
;
; Pin disabling:
;   1 to disable (0 is enabled, the default).
;
; HKR,%MixerDefaultsSubKeyName%,DisableWaveOut,                    1, 1
; HKR,%MixerDefaultsSubKeyName%,DisablePCBeep,                     1, 1
; HKR,%MixerDefaultsSubKeyName%,DisablePhone,                      1, 1
; HKR,%MixerDefaultsSubKeyName%,DisableMIC,                        1, 1
; HKR,%MixerDefaultsSubKeyName%,DisableLineIn,                     1, 1
; HKR,%MixerDefaultsSubKeyName%,DisableCDIn,                       1, 1
; HKR,%MixerDefaultsSubKeyName%,DisableVideo,                      1, 1
; HKR,%MixerDefaultsSubKeyName%,DisableAux,                        1, 1
; HKR,%MixerDefaultsSubKeyName%,DisableSurround,                   1, 1
; HKR,%MixerDefaultsSubKeyName%,DisableCenter,                     1, 1
; HKR,%MixerDefaultsSubKeyName%,DisableLFE,                        1, 1
; HKR,%MixerDefaultsSubKeyName%,Disable3DControl,                  1, 1
; HKR,%MixerDefaultsSubKeyName%,DisableStereoVirtual,              1, 1
; HKR,%MixerDefaultsSubKeyName%,DisableMonoVirtual,                1, 1
; HKR,%MixerDefaultsSubKeyName%,DisableStereo2Virtual,             1, 1
; HKR,%MixerDefaultsSubKeyName%,DisableMono2Virtual,                1, 1
HKR,%MixerDefaultsSubKeyName%,DisableHeadphone,                    1, 1
HKR,%MixerDefaultsSubKeyName%,DisableLnlvl,                        1, 1
HKR,%MixerDefaultsSubKeyName%,DisableWaveIn2,                      1, 1
; HKR,%MixerDefaultsSubKeyName%,DisableMonoOut,                    1, 1
; HKR,%MixerDefaultsSubKeyName%,DisablePeakmeters,                 1, 1
;
; Mixer control initial values:
;
; HKR,%MixerDefaultsSubKeyName%,WaveOutVolume,                     1, 00 ,80, 01, 00       ; (ffdd8000-c0000), (5 bit controls).
; HKR,%MixerDefaultsSubKeyName%,WaveOutMute,                       1, 0                    ; 0, unmuted, 1 muted
; HKR,%MixerDefaultsSubKeyName%,PCBeepVolume,                      1, 00, 00, 00, 00       ; (ffd30000-0), (4 bit control).
; HKR,%MixerDefaultsSubKeyName%,PCBeepVolumeInc,                   1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,PCBeepMute,                        1, 0                    ; 0, unmuted, 1 muted
; HKR,%MixerDefaultsSubKeyName%,PCBeepMuteInc,                     1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,PhoneVolume,                       1, 00, 00, 00, 00       ; (ffdd8000-c0000),   (5 bit control).
; HKR,%MixerDefaultsSubKeyName%,PhoneVolumeInc,                    1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,PhoneMute,                         1, 1                    ; 0, unmuted, 1 muted
; HKR,%MixerDefaultsSubKeyName%,PhoneMuteInc,                      1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,MICSelect,                         1, 0
; HKR,%MixerDefaultsSubKeyName%,MICBoost,                          1, 0
; HKR,%MixerDefaultsSubKeyName%,MICVolume,                         1, 00, 00, 00, 00       ; (ffdd8000-c0000),   (5 bit control).
; HKR,%MixerDefaultsSubKeyName%,MICVolumeInc,                      1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,MICMute,                           1, 1                    ; 0, unmuted, 1 muted
; HKR,%MixerDefaultsSubKeyName%,MICMuteInc,                        1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,LineInVolume,                      1, 00, 00, 00, 00       ; (ffdd8000-c0000),   (5 bit controls).
; HKR,%MixerDefaultsSubKeyName%,LineInVolumeInc,                   1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,LineInMute,                        1, 1                    ; 0, unmuted, 1 muted
; HKR,%MixerDefaultsSubKeyName%,LineInMuteInc,                     1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,CDVolume,                          1, 00, 00, 00, 00       ; (ffdd8000-c0000),   (5 bit controls).
; HKR,%MixerDefaultsSubKeyName%,CDVolumeInc,                       1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,CDMute,                            1, 0                    ; 0, unmuted, 1 muted
; HKR,%MixerDefaultsSubKeyName%,CDMuteInc,                         1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,VideoVolume,                       1, 00, 00, 00, 00       ; (ffdd8000-c0000),   (5 bit controls).
; HKR,%MixerDefaultsSubKeyName%,VideoVolumeInc,                    1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,VideoMute,                         1, 1                    ; 0, unmuted, 1 muted
; HKR,%MixerDefaultsSubKeyName%,VideoMuteInc,                      1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,AuxVolume,                         1, 00, 00, 00, 00       ; (ffdd8000-c0000),   (5 bit controls).
; HKR,%MixerDefaultsSubKeyName%,AuxVolumeInc,                      1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,AuxMute,                           1, 1                    ; 0, unmuted, 1 muted
; HKR,%MixerDefaultsSubKeyName%,AuxMuteInc,                        1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,SurroundVolume,                    1, 00, c0, e8, ff       ; (ffd18000-0), (5 bit controls).
; HKR,%MixerDefaultsSubKeyName%,SurroundVolumeInc,                 1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,SurroundMute,                      1, 0                    ; 0, unmuted, 1 muted
; HKR,%MixerDefaultsSubKeyName%,SurroundMuteInc,                   1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,CenterVolume,                      1, 00, c0, e8, ff       ; (ffd18000-0), (5 bit controls).
; HKR,%MixerDefaultsSubKeyName%,CenterVolumeInc,                   1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,CenterMute,                        1, 0                    ; 0, unmuted, 1 muted
; HKR,%MixerDefaultsSubKeyName%,CenterMuteInc,                     1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,LFEVolume,                         1, 00, c0, e8, ff       ; (ffd18000-0), (5 bit controls).
; HKR,%MixerDefaultsSubKeyName%,LFEVolumeInc,                      1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,LFEMute,                           1, 0                    ; 0, unmuted, 1 mute
; HKR,%MixerDefaultsSubKeyName%,LFEMuteInc,                        1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,3DDepthControl,                    1, 00, 80, 04, 00       ; (0-90000), 50%: 48000             (2 bit control).
; HKR,%MixerDefaultsSubKeyName%,3DDepthEnable,                     1, 1                    ; (inverted to match "Mute", 0 enabled, 1 disabled)
; HKR,%MixerDefaultsSubKeyName%,MasterVolume,                      1, 00, c0, e8, ff       ; (ffd18000-0), (5 bit controls).
; HKR,%MixerDefaultsSubKeyName%,MasterVolumeInc,                   1, 0                    ; 0, instantaneous, 1 incremental
HKR,%MixerDefaultsSubKeyName%,MasterMute,                          1, 0                    ; 0, unmuted, 1 muted
; HKR,%MixerDefaultsSubKeyName%,MasterMuteInc,                     1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,HeadphoneVolume,                   1, 00, c0, e8, ff       ; (ffd18000-0), 50%: ffe8c000       (5 bit controls).
; HKR,%MixerDefaultsSubKeyName%,HeadphoneVolumeInc,                1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,HeadphoneMute,                     1, 0                    ; 0, unmuted, 1 muted
; HKR,%MixerDefaultsSubKeyName%,HeadphoneMuteInc,                  1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,TrueLevelVolume,                   1, 00, c0, e8, ff       ; (ffd18000-0), 50%: ffe8c000       (5 bit controls).
; HKR,%MixerDefaultsSubKeyName%,TrueLevelVolumeInc,                1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,TrueLevelMute,                     1, 0                    ; 0, unmuted, 1 muted
; HKR,%MixerDefaultsSubKeyName%,TrueLevelMuteInc,                  1, 0                    ; 0, instantaneous, 1 incremental
; HKR,%MixerDefaultsSubKeyName%,MonoOutMux,                        1, 00, 00, 00, 00                    ; MonoOutMux selection values: (0: MIC), (1: MonoMix).
; HKR,%MixerDefaultsSubKeyName%,MICAtMonoOutVolume,                1, 00, c0, e8, ff       ; (ffd18000-0), 50%: ffe8c000       (5 bit controls).
; HKR,%MixerDefaultsSubKeyName%,MonoMixerAtMonoOutVolume,          1, 00, c0, e8, ff       ; (ffd18000-0), 50%: ffe8c000       (5 bit controls).
; HKR,%MixerDefaultsSubKeyName%,MICAtMonoOutMute,                  1, 0                    ; 0, unmuted, 1 muted
; HKR,%MixerDefaultsSubKeyName%,MonoMixerAtMonoOutMute,            1, 0                    ; 0, unmuted, 1 muted
; HKR,%MixerDefaultsSubKeyName%,WaveInMux,                         1, 00, 00, 00, 00       ; WaveInMux selection values: (0: MIC), (1: CD), (2: Video), (3: Aux), (4: LineIn), (5: StereoMix), (6: MonoMix), (7: Phone).
; HKR,%MixerDefaultsSubKeyName%,PhoneAtRecMuxVolume,               1, 00, 40, b0, 00       ; (0-168000), 50%: b4000            (4 bit controls).
; HKR,%MixerDefaultsSubKeyName%,MICAtRecMuxVolume,                 1, 00, 40, b0, 00       ; (0-168000), 50%: b4000            (4 bit controls).
; HKR,%MixerDefaultsSubKeyName%,CDAtRecMuxVolume,                  1, 00, 40, b0, 00       ; (0-168000), 50%: b4000            (4 bit controls).
; HKR,%MixerDefaultsSubKeyName%,VideoAtRecMuxVolume,               1, 00, 40, b0, 00       ; (0-168000), 50%: b4000            (4 bit controls).
; HKR,%MixerDefaultsSubKeyName%,AuxAtRecMuxVolume,                 1, 00, 40, b0, 00       ; (0-168000), 50%: b4000            (4 bit controls).
; HKR,%MixerDefaultsSubKeyName%,LineInAtRecMuxVolume,              1, 00, 40, b0, 00       ; (0-168000), 50%: b4000            (4 bit controls).
; HKR,%MixerDefaultsSubKeyName%,StereoMixAtRecMuxVolume,           1, 00, 40, b0, 00       ; (0-168000), 50%: b4000            (4 bit controls).
; HKR,%MixerDefaultsSubKeyName%,MonoMixAtRecMuxVolume,             1, 00, 40, b0, 00       ; (0-168000), 50%: b4000            (4 bit controls).
; HKR,%MixerDefaultsSubKeyName%,PhoneAtRecMuxMute,                 1, 0                    ; 0, unmuted, 1 muted
; HKR,%MixerDefaultsSubKeyName%,MICAtRecMuxMute,                   1, 0                    ; 0, unmuted, 1 muted
; HKR,%MixerDefaultsSubKeyName%,CDAtRecMuxMute,                    1, 0                    ; 0, unmuted, 1 muted
; HKR,%MixerDefaultsSubKeyName%,PhoneAtRecMuxMute,                 1, 0                    ; 0, unmuted, 1 muted
; HKR,%MixerDefaultsSubKeyName%,VideoAtRecMuxMute,                 1, 0                    ; 0, unmuted, 1 muted
; HKR,%MixerDefaultsSubKeyName%,LineInAtRecMuxMute,                1, 0                    ; 0, unmuted, 1 muted
; HKR,%MixerDefaultsSubKeyName%,StereoMixAtRecMuxMute,             1, 0                    ; 0, unmuted, 1 muted
; HKR,%MixerDefaultsSubKeyName%,MonoMixAtRecMuxMute,               1, 0                    ; 0, unmuted, 1 muted
; HKR,%MixerDefaultsSubKeyName%,MultiChannelEnable,                1, 0                    ; not enabled
; HKR,%MixerDefaultsSubKeyName%,CPL_SpdifTransmitterEnabledByUser,                       1, 0                    ; not enabled
; HKR,%MixerDefaultsSubKeyName%,GPIOControl,                       1, 0                    ; not enabled
;
; Other driver configuration entries.
; HKR,%ConfigurationsSubKeyName%,PCMVolumeFixedLevel,              1, 08, 08
; HKR,%ConfigurationsSubKeyName%,EmulateAllMasters,                1, 0
; HKR,%ConfigurationsSubKeyName%,DisableMicFromPlayback,           1, 0
; HKR,%ConfigurationsSubKeyName%,MasterControlsAux,                1, 1
; HKR,%ConfigurationsSubKeyName%,MasterControlsMono,               1, 1
; HKR,%ConfigurationsSubKeyName%,MICBoost30dB,                     1, 0     ; prefer 30dB to 20dB Boost on MIC if available.
; HKR,%ConfigurationsSubKeyName%,DCRecordBias,                     1, 10, 00, 00, 00
; HKR,%ConfigurationsSubKeyName%,FadeAudio,                        1, 1
; HKR,%ConfigurationsSubKeyName%,ActiveMuteDelayEnabled,           1, 1     ; If FadeAudio, zipper noise mute of PCM is deferred until signal fade has completed.
; HKR,%ConfigurationsSubKeyName%,MixerIncrementMicroSeconds,       1, d0, 07, 00, 00    ; 2000 uS delay on incremental mixer control updates (500 uS minimum enforced).
; HKR,%ConfigurationsSubKeyName%,SPDIFOutputDisable,               1, 0
; HKR,%ConfigurationsSubKeyName%,DisableNonPCM,                    1, 0
; HKR,%ConfigurationsSubKeyName%,EnableNonPCMOnWin2K,              1, 0
; HKR,%ConfigurationsSubKeyName%,SPDIFMutesMaster,           	   1, 0
; HKR,%ConfigurationsSubKeyName%,SPDIFMutesInactiveMaster,         1, 0
; HKR,%ConfigurationsSubKeyName%,SPDIFAssertsPR6,           	   1, 0
; HKR,%ConfigurationsSubKeyName%,MasterControlsSPDIFPCM,           1, 0
; HKR,%ConfigurationsSubKeyName%,DisableSPDIFControl,              1, 0
; HKR,%ConfigurationsSubKeyName%,EnableVRA,                        1, 0
;       VRA Disable bit positions:  D6: 8KHz, D5: 11.025KHz, D4: 16KHz, D3: 22.050KHz, D2: 32KHz, D1: 44.1KHz, D0: 48KHz
;       (D0 will be ignored).
; HKR,%ConfigurationsSubKeyName%,ADCVRADisables,                   1, 00, 00, 00, 00
; HKR,%ConfigurationsSubKeyName%,DACVRADisables,                   1, 00, 00, 00, 00
; HKR,%ConfigurationsSubKeyName%,MultiChannelDisable,              1, 0
; HKR,%ConfigurationsSubKeyName%,DisableMultiChannelControl,       1, 0
; HKR,%ConfigurationsSubKeyName%,SpeakerAutoDetection,             1, 0
; HKR,%ConfigurationsSubKeyName%,SpeakerDetectionInput,            1, 0		; Record mux selection values: (0: MIC), (1: CD), (2: Video), (3: Aux), (4: LineIn), (5: StereoMix), (6: MonoMix), (7: Phone).
; HKR,%ConfigurationsSubKeyName%,SpeakerDetectionAltMIC,           1, 0		; Use Alternate MIC if MIC selected as speaker detection input.
; HKR,%ConfigurationsSubKeyName%,SpeakerDetectionOutputAux,        1, 0		; Use Aux Out, else Line Out.
;       Speaker Auto detection threshold expressed as signed, 16 bit signal value (should be positive), 0 - 32767.
; HKR,%ConfigurationsSubKeyName%,SpeakerDetectionThreshold,        1, 0a, 00
; HKR,%ConfigurationsSubKeyName%,SpeakerDetectionRecordOnsetMilliSeconds,	1, 02
; HKR,%ConfigurationsSubKeyName%,SpeakerDetectionSamplingDelayMilliSeconds,	1, 04
; 		Enables jack sensing.
; HKR,%ConfigurationsSubKeyName%,GPIOJackSenseEnable,         	   1, 0
;       The default poll time for GPIO changes is 50 milliseconds.
; HKR,%ConfigurationsSubKeyName%,GPIOPollTimeMilliSeconds,         1, 32, 00
;       ORs SPDIF control with "DRM Digital Disable State" GPO.
; HKR,%ConfigurationsSubKeyName%,GPIOSPDIFControl,                 1, 0
;
;       GPIO actions are expressed as a binary string, a sequence of one or more 4-BYTE tuplets (beyond
;       the initial "1" type value required for registry entry). The 4 fields (each a BYTE in length) in each tuplet are:
;       { (Codec CID), (GPIO pin number), (GPIO action code), (Pin assertion sense) }
;
;       The "Codec CID" must match a recognized CODEC (by CID) on the AC97 link, and the "GPIO pin number"
;       must be a valid GPIO pin index for that CODEC.  If GPIO is enabled, there must be at least one
;       well-formed specification.
;
;       The valid values for "GPIO action code" (and implicit directions, GPI or GPO) are:
;
;           0       Disable software equalization (GPIDisableSoftwareEQ)        (GPI)
;           1       Mute master volume            (GPIMuteMasterVolume)         (GPI)
;           2       DRM Digital Disable State     (GPODRMDigitalDisable)        (GPO)
;
;       The "Pin assertion sense" maps the CODEC pin state to the logical assertion state of the action;
;       0 means the action is asserted on a sensed (or driven for GPO) CODEC pin value 0, non-zero means
;       asserted on sensed (driven) CODEC pin value 1.
;
; HKR,%ConfigurationsSubKeyName%,GPIOActions,                      1, 00, 00, 00, 00
;
; 		Delay (in uS) after RESET# deassertion before continued processing.
; HKR,%ConfigurationsSubKeyName%,CodecColdResetWaitMicroSeconds,   1, dc, 05, 00, 00
;
; HKR,%ConfigurationsSubKeyName%,DisableEQ,                        1, 0
;
; HKR,%ConfigurationsSubKeyName%,render_taps,                      1, 0b, 00, 00, 00
; HKR,%ConfigurationsSubKeyName%,render_roll_off,                  1, b6, 03, 00, 00
; HKR,%ConfigurationsSubKeyName%,render_beta,                      1, 28, 23, 00, 00
; HKR,%ConfigurationsSubKeyName%,capture_taps,                     1, 0b, 00, 00, 00
; HKR,%ConfigurationsSubKeyName%,capture_roll_off,                 1, b6, 03, 00, 00
; HKR,%ConfigurationsSubKeyName%,capture_beta,                     1, 28, 23, 00, 00

HKR,%ConfigurationsSubKeyName%,EnableExtAmpControl,                  1, 1
HKR,%ConfigurationsSubKeyName%,ExtAmpPowerDownTimeInMCS,             0x00010001, 5000
HKR,%ConfigurationsSubKeyName%,ExtAmpPowerUpTimeInMCS,               0x00010001, 5000
HKR,%ConfigurationsSubKeyName%,CodecPowerUpDelayInMCS,             0x00010001, 1000
;HKR,%ConfigurationsSubKeyName%,EnableVrefPowerDown,               1, 1
;HKR,%ConfigurationsSubKeyName%,VrefPowerDownTimeInMS,             0x00010001, 6000 ;6 seconds

; HKR,%ConfigurationsSubKeyName%,ModemInhibitsD3RST,               1, 1


[Strings]
SGTML="SigmaTel"
SgtmlMfg="SigmaTel"

STAC97.DeviceDesc="Audio controller - SigmaTel CODEC"
STAC97.DeviceDescSis961="SigmaTel C-Major Audio"

STAC97.Wave.szPname="SigmaTel Audio"
STAC97.AlternateWave.szPname="SigmaTel Alternate"
STAC97.Topology.szPname="SigmaTel"

SndVolSigKey="Software\Microsoft\Windows\CurrentVersion\Applets\Volume Control\SigmaTel Audio"

MediaCategories="SYSTEM\CurrentControlSet\Control\MediaCategories"

WDM_MIDI="WDM-based devices"

MixerDefaultsSubKeyName="Settings"
ConfigurationsSubKeyName="Settings"

Proxy.CLSID="{17CCA71B-ECD7-11D0-B908-00A0C9223196}"
KSCATEGORY_AUDIO="{6994AD04-93EF-11D0-A3CC-00A0C9223196}"
KSCATEGORY_RENDER="{65E8773E-8F56-11D0-A3B9-00A0C9223196}"
KSCATEGORY_CAPTURE="{65E8773D-8F56-11D0-A3B9-00A0C9223196}"
KSNAME_Wave="Wave"
KSNAME_AlternateWave="AlternateWave"
KSNAME_Topology="Topology"
KSNAME_UART="UART"
STAC97.UART.szPname="MIDI External Port"

STAC97.SvcDesc = "Audio Driver (WDM) - SigmaTel CODEC"

;; Nodes (non-localizeable)
STAC97GUID.PhoneVolume          ="{981DFEA0-27DB-11d3-99FC-00500483AC28}"
STAC97GUID.PhoneMute            ="{981DFEA1-27DB-11d3-99FC-00500483AC28}"
STAC97GUID.LineInMute           ="{981DFEA2-27DB-11d3-99FC-00500483AC28}"
STAC97GUID.MainMix              ="{981DFEA3-27DB-11d3-99FC-00500483AC28}"
STAC97GUID.3DBypass             ="{981DFEA4-27DB-11d3-99FC-00500483AC28}"
STAC97GUID.3DEnable             ="{981DFEA5-27DB-11d3-99FC-00500483AC28}"
STAC97GUID.BeepMix              ="{981DFEA6-27DB-11d3-99FC-00500483AC28}"
STAC97GUID.HPVolume             ="{981DFEA7-27DB-11d3-99FC-00500483AC28}"
STAC97GUID.HPMute               ="{981DFEA8-27DB-11d3-99FC-00500483AC28}"
STAC97GUID.LnlvlVolume          ="{301892ac-2f58-41c7-88b4-4c1d72501c83}"
STAC97GUID.LnlvlMute            ="{c5cb62ac-f62f-4569-b66b-6a1d3afe3388}"
STAC97GUID.MonoOutSelect        ="{981DFEA9-27DB-11d3-99FC-00500483AC28}"
STAC97GUID.WaveInSelect         ="{981DFEAA-27DB-11d3-99FC-00500483AC28}"
STAC97GUID.WaveIn2Select        ="{A514AD4E-CFB5-4ecc-9691-36494FBE0481}"
STAC97GUID.MasterInVolume       ="{981DFEAB-27DB-11d3-99FC-00500483AC28}"
STAC97GUID.MasterInMute         ="{981DFEAC-27DB-11d3-99FC-00500483AC28}"
STAC97GUID.MicInVolume          ="{981DFEAD-27DB-11d3-99FC-00500483AC28}"
STAC97GUID.MicInMute            ="{981DFEAE-27DB-11d3-99FC-00500483AC28}"
STAC97GUID.SurroundVolume       ="{81FBB14B-1BEE-4bf5-92EE-FFC4F75F326D}"
STAC97GUID.SurroundMute         ="{22654FBC-AC8F-4224-B19F-D858D2E10BDD}"
STAC97GUID.CenterVolume         ="{2D97372F-9CF6-4fd6-9E56-C68BACDF360D}"
STAC97GUID.CenterMute           ="{BEEF51ED-1041-43f8-9B96-5863D0A9342D}"
STAC97GUID.LFEVolume            ="{B60C4274-3BFD-430b-8364-D947E7D304B1}"
STAC97GUID.LFEMute              ="{4A4D9210-C780-4768-BFD2-525FDBF4FCB4}"
STAC97GUID.DigitalEnable        ="{56D8C1D0-58FB-4927-9CD2-8E3BD3E5A922}"
STAC97GUID.MultiChannelEnable   ="{A9D8349B-45CC-4A0B-97A2-D6AC7738F27D}"
STAC97GUID.GPIOControl          ="{88E542C4-1540-4a40-95D1-8CCC9A4B6245}"
STAC97GUID.HPOutPin             ="{981DFEB1-27DB-11d3-99FC-00500483AC28}"
STAC97GUID.LnlvlOutPin          ="{5A9EBEC6-FCA2-4fcd-AB11-04D6C3C6266A}"
STAC97GUID.Mic2Volume           ="{D68EA4BA-4E5B-45c4-9E80-AE7A959B969D}"
STAC97GUID.LineIn2Volume        ="{DD5102D5-9931-484c-8B47-FB9B75FE63A2}"
STAC97GUID.Mic2Pin              ="{A72A6A9C-896A-45ce-AD88-6BB096B11B36}"
STAC97GUID.LineIn2Pin           ="{CC57D9E2-9750-4b74-B509-41B9B30DC0B5}"
STAC97GUID.MonoMuteInMasterAdvanced="{A601A3BC-066E-4800-8922-6772422C0F18}"
STAC97GUID_ALTNAME.PcSpeaker    ="{88C02F6A-D1E7-4fe3-A506-9E0AE51D7820}"

;; Nodes (localizeable)
STAC97Node.PhoneVolume          ="Phone Volume"
STAC97Node.PhoneMute            ="Phone Mute"
STAC97Node.LineInMute           ="LineIn Mute"
STAC97Node.MainMix              ="Main Mix"
STAC97Node.3DBypass             ="3D Bypass"
STAC97Node.3DEnable             ="3D Enable"
STAC97Node.BeepMix              ="Beep Mix"
STAC97Node.HPVolume             ="Headphone Volume"
STAC97Node.HPMute               ="Headphone Mute"
STAC97Node.LnlvlVolume          ="Line Level Volume"
STAC97Node.LnlvlMute            ="Line Level Mute"
STAC97Node.MonoOutSelect        ="Mono Out Select"
STAC97Node.WaveInSelect         ="WaveIn Select"
STAC97Node.WaveIn2Select        ="Alt WaveIn Select"
STAC97Node.MasterInVolume       ="WaveIn Volume"
STAC97Node.MasterInMute         ="WaveIn Mute"
STAC97Node.MicInVolume          ="Mic In Volume"
STAC97Node.MicInMute            ="Mic In Mute"
STAC97Node.SurroundVolume       ="Surround Volume"
STAC97Node.SurroundMute         ="Surround Mute"
STAC97Node.CenterVolume         ="Center Volume"
STAC97Node.CenterMute           ="Center Mute"
STAC97Node.LFEVolume            ="LFE Volume"
STAC97Node.LFEMute              ="LFE Mute"
STAC97Node.DigitalEnable        ="Enable SPDIF"
STAC97Node.MultiChannelEnable   ="Enable Multi-Channel"
STAC97Node.GPIOControl          ="Enable SPDIF"
STAC97Node.Mic2Volume           ="Mic2 Volume"
STAC97Node.LineIn2Volume        ="LineIn2 Volume"
STAC97Pin.HPOutPin              ="Headphone"
STAC97Pin.LnlvlOutPin           ="Line Out"
STAC97Pin.Mic2Pin               ="Alt MIC"
STAC97Pin.LineIn2Pin            ="Alt LineIn"
STAC97Node.MonoMuteInMasterAdvanced="Mute Internal Speaker"
STAC97Pin.PcSpeaker             ="PC BEEP"
