-----------------------------------------------------------------
MicroTouch (TM) OEM Touch Screen Drivers and Utilities
For Windows (TM) XP Professional and Windows 2000 Professional
-----------------------------------------------------------------
Software Version 03.03.18P
Build Number:  03.03.18P / 3288 / G8515

This document supplements the information in the MicroTouch Near Field Imaging (TM) (NFI) Touch Screen System Software User's Guide for Windows XP and Windows 2000. This document covers the following topics:

1. Driver installation diskettes
2. Installing/upgrading the touch screen driver software
3. Concurrent mouse and touch screen operation
4. Online help "not enough memory" message
5. Uninstalling the touch screen driver software



1. DRIVER INSTALLATION DISKETTE
-------------------------------
This diskette is one of three that comprise the MicroTouch Near Field Imaging touch screen software running on Windows XP or Windows 2000 on the host computer.

The touch screen software includes the following files:

* setup.exe (Diskette 1)
* README_OEM_XP_2K.txt (Diskette 1)
* MAINDIR1.cab (Diskette 2)
* SYSDIR1.cab (Diskette 3)
* DRV32_1.cab (Diskette 3)
* MAINDIR2.cab (Diskette 3)

**NOTE**
Before installing the MicroTouch NFI touch screen software, uninstall any previously installed touch screen drivers.



2. INSTALLING/UPGRADING THE TOUCH SCREEN DRIVER SOFTWARE
--------------------------------------------------------

To install touch screen software for your MicroTouch NFI sensor onto your host computer (typically, on the hard disk drive C:\), you must have either Windows XP Professional or Windows 2000 Professional operating system running on the host computer. 

To install the driver for Windows XP/2000 operating systems from the floppy diskettes supplied with your monitor, follow these steps:

1. Close all open Windows programs.

2. Find the floppy disks with drivers for Windows XP/2000 operating systems, that includes setup.exe and insert it in the disk drive.

3. Copy all files from the floppy disks to the hard drive of your computer.

4. Run setup.exe from the hard drive. The installation Welcome window appears.

5. Follow the screen prompts to install the driver and then follow the on-screen instructions of the NFI Setup Wizard. **NOTE** When the Linearization Data Download dialog box appears, select Skip. Linearization data is built into the monitor at the factory.

6. When the NFI Setup Wizard finishes, the Install Successful window appears. It is not necessary to restart the computer. If the touch screen does not function, consult the Troubleshooting section of the monitor's installation guide. 



3. CONCURRENT MOUSE AND TOUCH SCREEN OPERATION
----------------------------------------------

Concurrent mouse and touch screen operation is supported by this driver. When the touch screen software has been successfully installed, both touch and mouse functions are available. 



4. ONLINE HELP "NOT ENOUGH MEMORY" MESSAGE
------------------------------------------
A Windows Help dialog box may appear if F1 (the online Help function) is selected while a touch screen driver dialog box is in focus on the desktop. The message in the dialog box reads: "There is not enough memory available for this task. Quit one or more programs to increase available memory, and then try again."

If this dialog box appears, select OK and ignore the message.

There is no online help for the Windows XP/2000 driver and the operating system misinterprets that fact as a memory error. For help with using and configuring the driver software, consult the MicroTouch Near Field Imaging (TM) (NFI) Software User's Guide for Windows XP and Windows 2000. This guide is available for download from www.3Mtouch.com.


5. UNINSTALLING THE WINDOWS XP/2000 TOUCH SCREEN DRIVER SOFTWARE
----------------------------------------------------------------

If it is ever necessary to uninstall the touch screen software for Windows XP or Windows 2000 operating systems, use the Windows Add/Remove Programs control panel:

1. From the Windows desktop, select Start, then Settings, then Control Panel, and then Add/Remove Programs. The Add/Remove Programs window appears.

2. Select the Universal Pointer Device Driver and then select the Change/Remove button. The Uninstall UPDD window appears.

3. Select Next. The Complete dialog box appears to confirm that the software is uninstalled.

4. Select Next to end the uninstall procedure.




-------------------------------------------------------------------
COPYRIGHT
This document is (c) 3M 2003. All rights reserved. 
Reproduction of the contents of this copyrighted manual in whole or in part, by any means, electronic or mechanical, for any purpose, without written permission of 3M Touch Systems, a subsidiary of 3M, is prohibited.

NOTICE
Given the variety of factors that can affect the use and performance of a 3M Touch Systems Product (the "Product"), including that solid state equipment has operation characteristics different from electromechanical equipment, some of which factors are uniquely within User's knowledge and control, it is essential that User evaluate the 3M Touch Systems Product and software to determine whether it is suitable for User's particular purpose and suitable for User's method of application. 3M Touch Systems' statements, engineering/technical information, and recommendations are provided for User's convenience, but their accuracy or completeness is not warranted. 3M Touch Systems products and software are not specifically designed for use in medical devices as defined by United States federal law. 3M Touch Systems products and software should not be used in such applications without 3M Touch Systems' express written consent. User should contact its sales representative if User's opportunity involves a medical device application.



IMPORTANT NOTICE TO PURCHASER
Specifications are subject to change without notice. These 3M Touch Systems' Products and software are warranted to meet their published specifications from the date of shipment and for the period stated in the specification. 3M Touch Systems makes no additional warranties, express or implied, including but not limited to any implied warranties of merchantability or fitness for a particular purpose. 
User is responsible for determining whether the 3M Touch Systems Products and software are fit for User's particular purpose and suitable for its method of production, including intellectual property liability for User's application. If the Product, software or software media is proven not to have met 3M Touch Systems' warranty, then 3M Touch Systems' sole obligation and User's and Purchaser's exclusive remedy, will be, at 3M Touch Systems' option, to repair or replace that Product quantity or software media or to refund its purchase price. 3M Touch Systems has no obligation under 3M Touch Systems' warranty for any Product, software or software media that has been modified or damaged through misuse, accident, neglect, or subsequent manufacturing operations or assemblies by anyone other than 3M Touch Systems. 3M Touch Systems shall not be liable in any action against it in any way related to the Products or software for any loss or damages, whether non-specified direct, indirect, special, incidental or consequential (including downtime, loss of profits or goodwill) regardless of the legal theory asserted.


Trademarks
MicroTouch and Near Field Imaging (NFI) are trademarks of 3M. 
All other brand and product names are trademarks or registered
trademarks of their respective companies and are hereby acknowledged.

--------------------------------------------------------------------
